Pulsar Operation Manual

## Commands A - E

`Axx` | Run Table | `ABCDE` | `Pattern/Table`
Table number specified by command value `xx`. It's possible to run a Table from within another table however: execution of Table will transfer to the new table. if a `Axx` command is specified in the `CM1` column, `CM2` won't be processed as the execution of the new Table will begin immediately.

`Bxx` | Select Vibrato | `ABC--` | `Pattern/Table`
Sets the Vibrato program, `xx` is index into Vibrato List

`Cxy` | Play Arpeggio 'Chord' | `ABCD-` | `Pattern/Table`
Play triad arpeggio for duration of note. Original note is root while 1st (`X`) and 2nd (`Y`) digits of the command value are the 2nd and 3rd notes of 'chord'. Note: arpeggio speed controlled by `PSWEEP-Q` value of current Instrument. The higher the `PSWEEP-Q` value, the faster the arpeggio cycles.

`Dxx` | Delay Note | `ABCDE` | `Pattern`
When placed on the same Pattern step as a note, the starting of the note will be delayed by `xx` ticks. If a new note is encountered before the number of ticks has passed the delayed note will be cancelled.

`Exx` | Select ADSR Envelope | `AB-D-` | `Pattern/Table`
Selects an ADSR Envelope from the Envelope List. `xx` is the desired Envelope number.
Track E: when used on Track E, this command sets the End Offset (`EN`) for the sample.